09:17:11 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3576	     24	   1576	   5176	   1438	RealOne.elf
Finished building: default.size.stdout
 
09:21:41 **** Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3576	     24	   1576	   5176	   1438	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:21:44 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3576	     24	   1576	   5176	   1438	RealOne.elf
Finished building: default.size.stdout
 
09:23:47 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3576	     24	   1576	   5176	   1438	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:25:15 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3632	     24	   1576	   5232	   1470	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
09:25:41 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3632	     24	   1576	   5232	   1470	RealOne.elf
Finished building: default.size.stdout
 
09:28:07 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3820	     20	   1572	   5412	   1524	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:30:04 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3820	     20	   1572	   5412	   1524	RealOne.elf
Finished building: default.size.stdout
 
09:33:28 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
../Core/Src/main.c: In function 'main':
../Core/Src/main.c:215:1: error: expected declaration or statement at end of input
 }
 ^
At top level:
../Core/Src/main.c:172:6: warning: 'SystemClock_Config_80M' defined but not used [-Wunused-function]
 void SystemClock_Config_80M(void)
      ^~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:107:6: warning: 'SystemClock_Config_24M_LSE' defined but not used [-Wunused-function]
 void SystemClock_Config_24M_LSE(void)
      ^~~~~~~~~~~~~~~~~~~~~~~~~~
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
"make -j8 all" terminated with exit code 2. Build might be incomplete.
09:35:25 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
../Core/Src/main.c: In function 'main':
../Core/Src/main.c:215:1: error: expected declaration or statement at end of input
 }
 ^
At top level:
../Core/Src/main.c:172:6: warning: 'SystemClock_Config_80M' defined but not used [-Wunused-function]
 void SystemClock_Config_80M(void)
      ^~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:107:6: warning: 'SystemClock_Config_24M_LSE' defined but not used [-Wunused-function]
 void SystemClock_Config_24M_LSE(void)
      ^~~~~~~~~~~~~~~~~~~~~~~~~~
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
"make -j8 all" terminated with exit code 2. Build might be incomplete.
09:39:04 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3780	     20	   1572	   5372	   14fc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
09:39:09 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3780	     20	   1572	   5372	   14fc	RealOne.elf
Finished building: default.size.stdout
 
09:44:36 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3780	     20	   1572	   5372	   14fc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:44:41 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3780	     20	   1572	   5372	   14fc	RealOne.elf
Finished building: default.size.stdout
 
09:47:38 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3780	     20	   1572	   5372	   14fc	RealOne.elf
Finished building: default.size.stdout
 
09:49:56 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3796	     20	   1572	   5388	   150c	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:51:43 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3796	     20	   1572	   5388	   150c	RealOne.elf
Finished building: default.size.stdout
 
09:52:52 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3796	     20	   1572	   5388	   150c	RealOne.elf
Finished building: default.size.stdout
 
09:56:36 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3756	     20	   1572	   5348	   14e4	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
09:57:22 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3756	     20	   1572	   5348	   14e4	RealOne.elf
Finished building: default.size.stdout
 
10:08:48 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3748	     20	   1572	   5340	   14dc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
10:08:57 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3748	     20	   1572	   5340	   14dc	RealOne.elf
Finished building: default.size.stdout
 
10:09:39 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3748	     20	   1572	   5340	   14dc	RealOne.elf
Finished building: default.size.stdout
 
10:26:55 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_hal_msp.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_hal_msp.d" -MT"Core/Src/stm32l4xx_hal_msp.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_hal_msp.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_it.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_it.d" -MT"Core/Src/stm32l4xx_it.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_it.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
10:27:43 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
10:28:07 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
10:28:17 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
10:28:21 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
10:28:38 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3976	     20	   1572	   5568	   15c0	RealOne.elf
Finished building: default.size.stdout
 
10:34:31 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3988	     20	   1572	   5580	   15cc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
10:38:01 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   3988	     20	   1572	   5580	   15cc	RealOne.elf
Finished building: default.size.stdout
 
10:00:06 **** Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
../Core/Src/main.c: In function 'RTC_wakeup_init':
../Core/Src/main.c:297:1: warning: implicit declaration of function 'LL_RTC_DisableWriteProtection'; did you mean 'LL_PWR_DisableSRAM2Retention'? [-Wimplicit-function-declaration]
 LL_RTC_DisableWriteProtection( RTC );
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~~~
 LL_PWR_DisableSRAM2Retention
../Core/Src/main.c:298:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_Disable'; did you mean 'LL_RCC_LSE_Disable'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_Disable( RTC );
 ^~~~~~~~~~~~~~~~~~~~~
 LL_RCC_LSE_Disable
../Core/Src/main.c:299:10: warning: implicit declaration of function 'LL_RTC_IsActiveFlag_WUTW'; did you mean 'LL_PWR_IsActiveFlag_WU1'? [-Wimplicit-function-declaration]
 while ( !LL_RTC_IsActiveFlag_WUTW( RTC ) )
          ^~~~~~~~~~~~~~~~~~~~~~~~
          LL_PWR_IsActiveFlag_WU1
../Core/Src/main.c:302:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_SetClock'; did you mean 'IS_RTC_WAKEUP_CLOCK'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_SetClock( RTC, LL_RTC_WAKEUPCLOCK_CKSPRE );
 ^~~~~~~~~~~~~~~~~~~~~~
 IS_RTC_WAKEUP_CLOCK
../Core/Src/main.c:302:30: error: 'LL_RTC_WAKEUPCLOCK_CKSPRE' undeclared (first use in this function); did you mean 'IS_RTC_WAKEUP_CLOCK'?
 LL_RTC_WAKEUP_SetClock( RTC, LL_RTC_WAKEUPCLOCK_CKSPRE );
                              ^~~~~~~~~~~~~~~~~~~~~~~~~
                              IS_RTC_WAKEUP_CLOCK
../Core/Src/main.c:302:30: note: each undeclared identifier is reported only once for each function it appears in
../Core/Src/main.c:304:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_SetAutoReload'; did you mean '__HAL_TIM_SetAutoreload'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_SetAutoReload( RTC, delay ); // 16 bits
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~
 __HAL_TIM_SetAutoreload
../Core/Src/main.c:305:1: warning: implicit declaration of function 'LL_RTC_ClearFlag_WUT'; did you mean 'LL_PWR_ClearFlag_WU1'? [-Wimplicit-function-declaration]
 LL_RTC_ClearFlag_WUT(RTC);
 ^~~~~~~~~~~~~~~~~~~~
 LL_PWR_ClearFlag_WU1
../Core/Src/main.c:306:1: warning: implicit declaration of function 'LL_RTC_EnableIT_WUT'; did you mean 'LL_DMA_EnableIT_HT'? [-Wimplicit-function-declaration]
 LL_RTC_EnableIT_WUT(RTC);
 ^~~~~~~~~~~~~~~~~~~
 LL_DMA_EnableIT_HT
../Core/Src/main.c:307:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_Enable'; did you mean 'LL_RCC_LSE_Enable'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_Enable(RTC);
 ^~~~~~~~~~~~~~~~~~~~
 LL_RCC_LSE_Enable
../Core/Src/main.c:308:1: warning: implicit declaration of function 'LL_RTC_EnableWriteProtection'; did you mean 'LL_PWR_EnableSRAM2Retention'? [-Wimplicit-function-declaration]
 LL_RTC_EnableWriteProtection(RTC);
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~~
 LL_PWR_EnableSRAM2Retention
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
"make -j8 all" terminated with exit code 2. Build might be incomplete.
10:58:21 **** Clean-only build of configuration Debug for project RealOne ****
make -j8 clean 
rm -rf *
 
10:58:22 **** Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.c:36:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.c:36:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.c:36:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal.c:36:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_dma_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash.c:90:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.c:87:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.c:87:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.c:87:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_exti.c:87:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.c:105:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.c:105:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.c:105:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_cortex.c:105:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ramfunc.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.c:63:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.c:63:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.c:63:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_flash_ex.c:63:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.c:106:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.c:106:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.c:106:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_gpio.c:106:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.c:308:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.c:308:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.c:308:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c.c:308:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_i2c_ex.c:50:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_pwr_ex.c:26:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.c:53:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.c:53:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.c:53:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc.c:53:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.c:27:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.c:27:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.c:27:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rcc_ex.c:27:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.c:182:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.c:182:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.c:182:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc.c:182:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.o"
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.c:112:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.c:112:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.c:112:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_rtc_ex.c:112:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.c:187:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.c:187:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.c:187:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim.c:187:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.c:80:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.c:80:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.c:80:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_hal_tim_ex.c:80:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.d" -MT"Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.o"
arm-none-eabi-gcc -mcpu=cortex-m4 -g3 -c -x assembler-with-cpp -MMD -MP -MF"Core/Startup/startup_stm32l476rgtx.d" -MT"Core/Startup/startup_stm32l476rgtx.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Startup/startup_stm32l476rgtx.o" "../Core/Startup/startup_stm32l476rgtx.s"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_exti.h:29,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_exti.h:29,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_exti.h:29,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_exti.h:29,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_exti.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:0:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:0:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:45,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_rtc.c:39:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc "../Core/Src/gpio.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/gpio.d" -MT"Core/Src/gpio.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/gpio.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_utils.h:41,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.c:20:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_utils.h:41,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.c:20:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_utils.h:41,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.c:20:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_utils.h:41,
                 from ../Drivers/STM32L4xx_HAL_Driver/Src/stm32l4xx_ll_utils.c:20:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_bus.h:46,
                 from ../Core/Src/gpio.c:4:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_bus.h:46,
                 from ../Core/Src/gpio.c:4:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_bus.h:46,
                 from ../Core/Src/gpio.c:4:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_bus.h:46,
                 from ../Core/Src/gpio.c:4:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Core/Src/stm32l4xx_hal_msp.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_hal_msp.d" -MT"Core/Src/stm32l4xx_hal_msp.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_hal_msp.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
arm-none-eabi-gcc "../Core/Src/stm32l4xx_it.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_it.d" -MT"Core/Src/stm32l4xx_it.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_it.o"
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Core/Src/syscalls.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/syscalls.d" -MT"Core/Src/syscalls.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/syscalls.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
arm-none-eabi-gcc "../Core/Src/sysmem.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/sysmem.d" -MT"Core/Src/sysmem.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/sysmem.o"
arm-none-eabi-gcc "../Core/Src/system_stm32l4xx.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/system_stm32l4xx.d" -MT"Core/Src/system_stm32l4xx.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/system_stm32l4xx.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
../Core/Src/main.c: In function 'RTC_wakeup_init':
../Core/Src/main.c:297:1: warning: implicit declaration of function 'LL_RTC_DisableWriteProtection'; did you mean 'LL_PWR_DisableSRAM2Retention'? [-Wimplicit-function-declaration]
 LL_RTC_DisableWriteProtection( RTC );
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~~~
 LL_PWR_DisableSRAM2Retention
../Core/Src/main.c:298:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_Disable'; did you mean 'LL_RCC_LSE_Disable'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_Disable( RTC );
 ^~~~~~~~~~~~~~~~~~~~~
 LL_RCC_LSE_Disable
../Core/Src/main.c:299:10: warning: implicit declaration of function 'LL_RTC_IsActiveFlag_WUTW'; did you mean 'LL_PWR_IsActiveFlag_WU1'? [-Wimplicit-function-declaration]
 while ( !LL_RTC_IsActiveFlag_WUTW( RTC ) )
          ^~~~~~~~~~~~~~~~~~~~~~~~
          LL_PWR_IsActiveFlag_WU1
../Core/Src/main.c:302:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_SetClock'; did you mean 'IS_RTC_WAKEUP_CLOCK'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_SetClock( RTC, LL_RTC_WAKEUPCLOCK_CKSPRE );
 ^~~~~~~~~~~~~~~~~~~~~~
 IS_RTC_WAKEUP_CLOCK
../Core/Src/main.c:302:30: error: 'LL_RTC_WAKEUPCLOCK_CKSPRE' undeclared (first use in this function); did you mean 'IS_RTC_WAKEUP_CLOCK'?
 LL_RTC_WAKEUP_SetClock( RTC, LL_RTC_WAKEUPCLOCK_CKSPRE );
                              ^~~~~~~~~~~~~~~~~~~~~~~~~
                              IS_RTC_WAKEUP_CLOCK
../Core/Src/main.c:302:30: note: each undeclared identifier is reported only once for each function it appears in
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Core/Src/system_stm32l4xx.c:92:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Core/Src/system_stm32l4xx.c:92:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Core/Src/system_stm32l4xx.c:92:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Drivers/CMSIS/Device/ST/STM32L4xx/Include/stm32l4xx.h:235,
                 from ../Core/Src/system_stm32l4xx.c:92:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
../Core/Src/main.c:304:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_SetAutoReload'; did you mean '__HAL_TIM_SetAutoreload'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_SetAutoReload( RTC, delay ); // 16 bits
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~
 __HAL_TIM_SetAutoreload
../Core/Src/main.c:305:1: warning: implicit declaration of function 'LL_RTC_ClearFlag_WUT'; did you mean 'LL_PWR_ClearFlag_WU1'? [-Wimplicit-function-declaration]
 LL_RTC_ClearFlag_WUT(RTC);
 ^~~~~~~~~~~~~~~~~~~~
 LL_PWR_ClearFlag_WU1
../Core/Src/main.c:306:1: warning: implicit declaration of function 'LL_RTC_EnableIT_WUT'; did you mean 'LL_DMA_EnableIT_HT'? [-Wimplicit-function-declaration]
 LL_RTC_EnableIT_WUT(RTC);
 ^~~~~~~~~~~~~~~~~~~
 LL_DMA_EnableIT_HT
../Core/Src/main.c:307:1: warning: implicit declaration of function 'LL_RTC_WAKEUP_Enable'; did you mean 'LL_RCC_LSE_Enable'? [-Wimplicit-function-declaration]
 LL_RTC_WAKEUP_Enable(RTC);
 ^~~~~~~~~~~~~~~~~~~~
 LL_RCC_LSE_Enable
../Core/Src/main.c:308:1: warning: implicit declaration of function 'LL_RTC_EnableWriteProtection'; did you mean 'LL_PWR_EnableSRAM2Retention'? [-Wimplicit-function-declaration]
 LL_RTC_EnableWriteProtection(RTC);
 ^~~~~~~~~~~~~~~~~~~~~~~~~~~~
 LL_PWR_EnableSRAM2Retention
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
make: *** Waiting for unfinished jobs....
"make -j8 all" terminated with exit code 2. Build might be incomplete.
10:59:57 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_hal_msp.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_hal_msp.d" -MT"Core/Src/stm32l4xx_hal_msp.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_hal_msp.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_it.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_it.d" -MT"Core/Src/stm32l4xx_it.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_it.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Src/stm32l4xx_hal_msp.c:23:0:
../Core/Inc/main.h:70:13: warning: 'RTC_wakeup_init' declared 'static' but never defined [-Wunused-function]
 static void RTC_wakeup_init( int delay );
             ^~~~~~~~~~~~~~~
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
In file included from ../Core/Src/stm32l4xx_it.c:22:0:
../Core/Inc/main.h:70:13: warning: 'RTC_wakeup_init' declared 'static' but never defined [-Wunused-function]
 static void RTC_wakeup_init( int delay );
             ^~~~~~~~~~~~~~~
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-size   RealOne.elf 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
   text	   data	    bss	    dec	    hex	filename
   4036	     20	   1572	   5628	   15fc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
11:00:17 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_hal_msp.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_hal_msp.d" -MT"Core/Src/stm32l4xx_hal_msp.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_hal_msp.o"
arm-none-eabi-gcc "../Core/Src/stm32l4xx_it.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/stm32l4xx_it.d" -MT"Core/Src/stm32l4xx_it.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/stm32l4xx_it.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_hal_msp.c:23:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/stm32l4xx_it.c:22:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4036	     20	   1572	   5628	   15fc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
11:02:22 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4036	     20	   1572	   5628	   15fc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
11:22:31 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4956	     20	   1572	   6548	   1994	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
11:25:55 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4972	     20	   1572	   6564	   19a4	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
11:26:16 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4972	     20	   1572	   6564	   19a4	RealOne.elf
Finished building: default.size.stdout
 
11:36:20 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
11:36:25 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
11:39:14 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
11:43:47 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
11:43:51 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
11:59:01 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4984	     20	   1572	   6576	   19b0	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
12:10:16 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4980	     20	   1572	   6572	   19ac	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
12:16:54 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
../Core/Src/main.c: In function 'main':
../Core/Src/main.c:141:5: error: expected '}' before 'else'
    }else{
     ^~~~
../Core/Src/main.c:145:5: error: expected ';' before '}' token
     }
     ^
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
"make -j8 all" terminated with exit code 2. Build might be incomplete.
12:17:48 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
../Core/Src/main.c: In function 'main':
../Core/Src/main.c:330:13: error: invalid storage class for function 'RTC_wakeup_init'
 static void RTC_wakeup_init( int delay )
             ^~~~~~~~~~~~~~~
../Core/Src/main.c:374:1: error: expected declaration or statement at end of input
 }
 ^
At top level:
../Core/Src/main.c:371:6: warning: 'RTC_WKUP_IRQHandler' defined but not used [-Wunused-function]
 void RTC_WKUP_IRQHandler()
      ^~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:359:6: warning: 'RTC_wakeup_init_from_stop' defined but not used [-Wunused-function]
 void RTC_wakeup_init_from_stop( int delay )
      ^~~~~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:348:6: warning: 'RTC_wakeup_init_from_standby_or_shutdown' defined but not used [-Wunused-function]
 void RTC_wakeup_init_from_standby_or_shutdown( int delay )
      ^~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:284:6: warning: 'SystemClock_Config_80M' defined but not used [-Wunused-function]
 void SystemClock_Config_80M(void)
      ^~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:219:6: warning: 'SystemClock_Config_24M_LSE' defined but not used [-Wunused-function]
 void SystemClock_Config_24M_LSE(void)
      ^~~~~~~~~~~~~~~~~~~~~~~~~~
../Core/Src/main.c:151:6: warning: 'SystemClock_Config_24M_LSE_FL3_VS2' defined but not used [-Wunused-function]
 void SystemClock_Config_24M_LSE_FL3_VS2(void){
      ^~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
make: *** [Core/Src/subdir.mk:38: Core/Src/main.o] Error 1
"make -j8 all" terminated with exit code 2. Build might be incomplete.
12:18:17 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4996	     20	   1572	   6588	   19bc	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
12:20:46 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4992	     20	   1572	   6584	   19b8	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
12:21:52 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4988	     20	   1572	   6580	   19b4	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
 
Finished building: RealOne.list
 
12:25:51 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   4992	     20	   1572	   6584	   19b8	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
12:27:22 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   5004	     20	   1572	   6596	   19c4	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
12:28:19 **** Incremental Build of configuration Debug for project RealOne ****
make -j8 all 
arm-none-eabi-gcc "../Core/Src/main.c" -mcpu=cortex-m4 -std=gnu11 -g3 '-DHSE_VALUE=8000000' '-DMSI_VALUE=4000000' '-DLSI_VALUE=32000' '-DHSE_STARTUP_TIMEOUT=100' '-DHSI_VALUE=16000000' -DDEBUG '-DLSE_STARTUP_TIMEOUT=5000' '-DLSE_VALUE=32768' '-DDATA_CACHE_ENABLE=1' -DUSE_HAL_DRIVER '-DVDD_VALUE=3300' '-DINSTRUCTION_CACHE_ENABLE=1' '-DEXTERNALSAI2_CLOCK_VALUE=2097000' -DSTM32L476xx -DUSE_FULL_LL_DRIVER '-DEXTERNALSAI1_CLOCK_VALUE=2097000' '-DPREFETCH_ENABLE=0' -c -I../Core/Inc -I../Drivers/STM32L4xx_HAL_Driver/Inc -I../Drivers/CMSIS/Device/ST/STM32L4xx/Include -I../Drivers/CMSIS/Include -I../Drivers/STM32L4xx_HAL_Driver/Inc/Legacy -O0 -ffunction-sections -fdata-sections -Wall -fstack-usage -MMD -MP -MF"Core/Src/main.d" -MT"Core/Src/main.o" --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -o "Core/Src/main.o"
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:183:0: warning: "VDD_VALUE" redefined
 #define  VDD_VALUE       3300U /*!< Value of VDD in mv */
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:186:0: warning: "PREFETCH_ENABLE" redefined
 #define  PREFETCH_ENABLE              0U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:187:0: warning: "INSTRUCTION_CACHE_ENABLE" redefined
 #define  INSTRUCTION_CACHE_ENABLE     1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30:0,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Core/Inc/stm32l4xx_hal_conf.h:188:0: warning: "DATA_CACHE_ENABLE" redefined
 #define  DATA_CACHE_ENABLE            1U
 
<command-line>:0:0: note: this is the location of the previous definition
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:64:0: warning: "RTC_INIT_MASK" redefined
  #define RTC_INIT_MASK                 0xFFFFFFFFU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:979:0: note: this is the location of the previous definition
 #define RTC_INIT_MASK                       0xFFFFFFFFu
 
In file included from ../Core/Inc/main.h:42:0,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_ll_rtc.h:65:0: warning: "RTC_RSF_MASK" redefined
  #define RTC_RSF_MASK                  0xFFFFFF5FU
 
In file included from ../Core/Inc/stm32l4xx_hal_conf.h:409:0,
                 from ../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal.h:30,
                 from ../Core/Inc/main.h:31,
                 from ../Core/Src/main.c:8:
../Drivers/STM32L4xx_HAL_Driver/Inc/stm32l4xx_hal_rtc.h:983:0: note: this is the location of the previous definition
 #define RTC_RSF_MASK                        (~(RTC_ISR_INIT | RTC_ISR_RSF))
 
arm-none-eabi-gcc -o "RealOne.elf" @"objects.list"   -mcpu=cortex-m4 -T"C:\Users\camer\Desktop\LoPoSo\RealOne\STM32L476RGTX_FLASH.ld" --specs=nosys.specs -Wl,-Map="RealOne.map" -Wl,--gc-sections -static --specs=nano.specs -mfpu=fpv4-sp-d16 -mfloat-abi=hard -mthumb -Wl,--start-group -lc -lm -Wl,--end-group
Finished building target: RealOne.elf
 
arm-none-eabi-objdump -h -S  RealOne.elf  > "RealOne.list"
arm-none-eabi-objcopy  -O binary  RealOne.elf  "RealOne.bin"
arm-none-eabi-size   RealOne.elf 
   text	   data	    bss	    dec	    hex	filename
   5008	     20	   1572	   6600	   19c8	RealOne.elf
Finished building: default.size.stdout
 
Finished building: RealOne.bin
Finished building: RealOne.list
 
 
