Component: ARM Compiler 5.06 update 7 (build 960) Tool: armlink [4d3601]

==============================================================================

Section Cross References

    driver_gpio.o(i.MyGPIO_Init) refers to driver_gpio.o(i.MyGPIO_Set) for MyGPIO_Set
    driver_gpio.o(i.MyGPIO_Toggle) refers to driver_gpio.o(i.MyGPIO_Reset) for MyGPIO_Reset
    driver_gpio.o(i.MyGPIO_Toggle) refers to driver_gpio.o(i.MyGPIO_Set) for MyGPIO_Set
    driver_timer.o(i.MyTimer_Active_IT) refers to driver_timer.o(i.__NVIC_EnableIRQ) for __NVIC_EnableIRQ
    driver_timer.o(i.MyTimer_Active_IT) refers to driver_timer.o(i.__NVIC_SetPriority) for __NVIC_SetPriority
    driver_timer.o(i.MyTimer_Active_IT) refers to driver_timer.o(.data) for IT_function_TIM1
    driver_timer.o(i.MyTimer_PWM_set_cycle) refers to ffltui.o(.text) for __aeabi_ui2f
    driver_timer.o(i.MyTimer_PWM_set_cycle) refers to fmul.o(.text) for __aeabi_fmul
    driver_timer.o(i.MyTimer_PWM_set_cycle) refers to ffixi.o(.text) for __aeabi_f2iz
    driver_timer.o(i.TIM1_TRG_COM_IRQHandler) refers to driver_timer.o(.data) for IT_function_TIM1
    driver_timer.o(i.TIM2_IRQHandler) refers to driver_timer.o(.data) for IT_function_TIM2
    driver_timer.o(i.TIM3_IRQHandler) refers to driver_timer.o(.data) for IT_function_TIM3
    driver_timer.o(i.TIM4_IRQHandler) refers to driver_timer.o(.data) for IT_function_TIM4
    driver_spi.o(i.SPI_rcv) refers to driver_spi.o(i.SPI_send) for SPI_send
    chavirement.o(i.chavirement_handler) refers to chavirement.o(i.lire) for lire
    chavirement.o(i.chavirement_init) refers to driver_gpio.o(i.MyGPIO_Init) for MyGPIO_Init
    chavirement.o(i.chavirement_init) refers to driver_spi.o(i.SPI_activate_clock) for SPI_activate_clock
    chavirement.o(i.chavirement_init) refers to driver_spi.o(i.SPI_init_master) for SPI_init_master
    chavirement.o(i.chavirement_init) refers to chavirement.o(i.ecrire) for ecrire
    chavirement.o(i.ecrire) refers to driver_spi.o(i.SPI_send) for SPI_send
    chavirement.o(i.lire) refers to driver_spi.o(i.SPI_send) for SPI_send
    chavirement.o(i.lire) refers to driver_spi.o(i.SPI_rcv) for SPI_rcv
    startup_stm32f10x_md.o(RESET) refers to startup_stm32f10x_md.o(STACK) for __initial_sp
    startup_stm32f10x_md.o(RESET) refers to startup_stm32f10x_md.o(.text) for Reset_Handler
    startup_stm32f10x_md.o(RESET) refers to driver_timer.o(i.TIM1_TRG_COM_IRQHandler) for TIM1_TRG_COM_IRQHandler
    startup_stm32f10x_md.o(RESET) refers to driver_timer.o(i.TIM2_IRQHandler) for TIM2_IRQHandler
    startup_stm32f10x_md.o(RESET) refers to driver_timer.o(i.TIM3_IRQHandler) for TIM3_IRQHandler
    startup_stm32f10x_md.o(RESET) refers to driver_timer.o(i.TIM4_IRQHandler) for TIM4_IRQHandler
    startup_stm32f10x_md.o(.text) refers to system_stm32f10x.o(i.SystemInit) for SystemInit
    startup_stm32f10x_md.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    system_stm32f10x.o(i.SetSysClock) refers to system_stm32f10x.o(i.SetSysClockTo72) for SetSysClockTo72
    system_stm32f10x.o(i.SystemCoreClockUpdate) refers to system_stm32f10x.o(.data) for SystemCoreClock
    system_stm32f10x.o(i.SystemInit) refers to system_stm32f10x.o(i.SetSysClock) for SetSysClock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000F) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$00000011) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry12b.o(.ARM.Collect$$$$0000000E) for __rt_lib_shutdown_fini
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    fmul.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    ffltui.o(.text) refers to fepilogue.o(.text) for _float_epilogue
    ffixi.o(.text) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_stm32f10x_md.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_stm32f10x_md.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to principal.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to principal.o(i.main) for main
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload


==============================================================================

Removing Unused input sections from the image.

    Removing driver_gpio.o(.rev16_text), (4 bytes).
    Removing driver_gpio.o(.revsh_text), (4 bytes).
    Removing driver_gpio.o(.rrx_text), (6 bytes).
    Removing driver_gpio.o(i.MyGPIO_Activate), (24 bytes).
    Removing driver_gpio.o(i.MyGPIO_Init), (166 bytes).
    Removing driver_gpio.o(i.MyGPIO_Read), (12 bytes).
    Removing driver_gpio.o(i.MyGPIO_Reset), (12 bytes).
    Removing driver_gpio.o(i.MyGPIO_Set), (8 bytes).
    Removing driver_gpio.o(i.MyGPIO_Toggle), (36 bytes).
    Removing driver_timer.o(.rev16_text), (4 bytes).
    Removing driver_timer.o(.revsh_text), (4 bytes).
    Removing driver_timer.o(.rrx_text), (6 bytes).
    Removing driver_timer.o(i.Activate_TIM), (40 bytes).
    Removing driver_timer.o(i.MyTimer_Active_IT), (148 bytes).
    Removing driver_timer.o(i.MyTimer_Base_Init), (18 bytes).
    Removing driver_timer.o(i.MyTimer_PWM), (192 bytes).
    Removing driver_timer.o(i.MyTimer_PWM_set_cycle), (132 bytes).
    Removing driver_timer.o(i.__NVIC_EnableIRQ), (34 bytes).
    Removing driver_timer.o(i.__NVIC_SetPriority), (40 bytes).
    Removing driver_spi.o(.rev16_text), (4 bytes).
    Removing driver_spi.o(.revsh_text), (4 bytes).
    Removing driver_spi.o(.rrx_text), (6 bytes).
    Removing driver_spi.o(i.SPI_activate_clock), (60 bytes).
    Removing driver_spi.o(i.SPI_init_master), (74 bytes).
    Removing driver_spi.o(i.SPI_rcv), (32 bytes).
    Removing driver_spi.o(i.SPI_send), (18 bytes).
    Removing chavirement.o(.rev16_text), (4 bytes).
    Removing chavirement.o(.revsh_text), (4 bytes).
    Removing chavirement.o(.rrx_text), (6 bytes).
    Removing chavirement.o(i.chavirement_handler), (42 bytes).
    Removing chavirement.o(i.chavirement_init), (92 bytes).
    Removing chavirement.o(i.ecrire), (28 bytes).
    Removing chavirement.o(i.lire), (32 bytes).
    Removing startup_stm32f10x_md.o(HEAP), (512 bytes).
    Removing system_stm32f10x.o(.rev16_text), (4 bytes).
    Removing system_stm32f10x.o(.revsh_text), (4 bytes).
    Removing system_stm32f10x.o(.rrx_text), (6 bytes).
    Removing system_stm32f10x.o(i.SystemCoreClockUpdate), (164 bytes).
    Removing system_stm32f10x.o(.data), (20 bytes).
    Removing fmul.o(.text), (100 bytes).
    Removing ffltui.o(.text), (10 bytes).
    Removing ffixi.o(.text), (50 bytes).
    Removing fepilogue.o(.text), (110 bytes).

43 unused section(s) (total 2276 bytes) removed from the image.
