# Static Call Graph - [NUCLEO-F103RB\NUCLEO-F103RB.axf]

# Static Call Graph for image NUCLEO-F103RB\NUCLEO-F103RB.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Nov 11 15:46:52 2020

### Maximum Stack Usage = 136 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ is_level_enough ⇒ get_battery_level ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SVC_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from mytimer.o(i.TIM1_UP_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from mytimer.o(i.TIM2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from mytimer.o(i.TIM3_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from mytimer.o(i.TIM4_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> get_battery_level

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> get_battery_level

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> get_battery_level

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> is_level_enough
  - >> get_battery_level

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cdcmple.o(.text), UNUSED)

  __aeabi_cdcmple (Thumb, 48 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> is_level_enough

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Called By]
  - >> get_battery_level

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text), UNUSED)

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> _double_epilogue

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_dmul

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  LL_ADC_Init (Thumb, 120 bytes, Stack size 16 bytes, stm32f1xx_ll_adc.o(i.LL_ADC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_Init
  [Calls]
  - >> LL_ADC_IsEnabled
  - >> assert_failed
  [Called By]
  - >> alimentation_init

  LL_ADC_REG_Init (Thumb, 454 bytes, Stack size 16 bytes, stm32f1xx_ll_adc.o(i.LL_ADC_REG_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = LL_ADC_REG_Init
  [Calls]
  - >> LL_ADC_IsEnabled
  - >> assert_failed
  [Called By]
  - >> alimentation_init

  LL_Init1msTick (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_ll_utils.o(i.LL_Init1msTick))
  [Called By]

  - >> SystemClock_Config

  LL_SetSystemCoreClock (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_ll_utils.o(i.LL_SetSystemCoreClock))
  [Called By]

  - >> SystemClock_Config

  SystemClock_Config (Thumb, 226 bytes, Stack size 8 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemClock_Config
  [Calls]
  - >> LL_SetSystemCoreClock
  - >> LL_Init1msTick
  [Called By]
  - >> main

  SystemInit (Thumb, 70 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  TIM1_UP_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, mytimer.o(i.TIM1_UP_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM1_UP_IRQHandler
  [Calls]
  - >> LL_TIM_ClearFlag_UPDATE
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  TIM2_IRQHandler (Thumb, 18 bytes, Stack size 8 bytes, mytimer.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM2_IRQHandler
  [Calls]
  - >> LL_TIM_ClearFlag_UPDATE
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, mytimer.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM3_IRQHandler
  [Calls]
  - >> LL_TIM_ClearFlag_UPDATE
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, mytimer.o(i.TIM4_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM4_IRQHandler
  [Calls]
  - >> LL_TIM_ClearFlag_UPDATE
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  alimentation_init (Thumb, 146 bytes, Stack size 80 bytes, alimentation.o(i.alimentation_init))
  [Stack]

  - Max Depth = 96
  - Call Chain = alimentation_init ⇒ LL_ADC_REG_Init
  [Calls]
  - >> LL_ADC_REG_Init
  - >> LL_ADC_Init
  [Called By]
  - >> main

  assert_failed (Thumb, 4 bytes, Stack size 0 bytes, main.o(i.assert_failed))
  [Called By]

  - >> LL_ADC_REG_Init
  - >> LL_ADC_Init

  get_battery_level (Thumb, 166 bytes, Stack size 32 bytes, alimentation.o(i.get_battery_level))
  [Stack]

  - Max Depth = 120
  - Call Chain = get_battery_level ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> is_level_enough
  - >> main

  is_level_enough (Thumb, 32 bytes, Stack size 16 bytes, alimentation.o(i.is_level_enough))
  [Stack]

  - Max Depth = 136
  - Call Chain = is_level_enough ⇒ get_battery_level ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_cdcmple
  - >> get_battery_level
  [Called By]
  - >> main

  main (Thumb, 28 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 136
  - Call Chain = main ⇒ is_level_enough ⇒ get_battery_level ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> is_level_enough
  - >> get_battery_level
  - >> alimentation_init
  - >> SystemClock_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  LL_TIM_ClearFlag_UPDATE (Thumb, 8 bytes, Stack size 0 bytes, mytimer.o(i.LL_TIM_ClearFlag_UPDATE))
  [Called By]

  - >> TIM4_IRQHandler
  - >> TIM3_IRQHandler
  - >> TIM2_IRQHandler
  - >> TIM1_UP_IRQHandler

  LL_ADC_IsEnabled (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_ll_adc.o(i.LL_ADC_IsEnabled))
  [Called By]

  - >> LL_ADC_REG_Init
  - >> LL_ADC_Init

  ### Undefined Global Symbols