


ARM Macro Assembler    Page 1 


    1 00000000                 PRESERVE8
    2 00000000                 THUMB
    3 00000000                 include          DriverJeuLaser.inc
    1 00000000         
    2 00000000         ; Bibliotheque DriverJeuLaser (ancienne gassp72 adaptée 
                       2021 - TR)
    3 00000000         ; Accès en aux fonctions suivantes :
    4 00000000         ; GPIO :
    5 00000000         ; GPIOA_Set(char Broche), GPIOB_Set(char Broche), GPIOC_
                       Set(char Broche)
    6 00000000         ; GPIOA_Clear(char Broche), GPIOB_Clear(char Broche), GP
                       IOC_Clear(char Broche)
    7 00000000         
    8 00000000         ; PWM :
    9 00000000         ;/**
   10 00000000         ; * @brief  Fixe une valeur de PWM, Val, en tick horloge
                       . La rapport cyclique effectif
   11 00000000         ; * est donc : rcy = Thaut_ticks / Periode_ticks
   12 00000000         ; * @note   spécifique Jeu Laser, PWM liée exclusivement
                        au TIM3, chan3
   13 00000000         ; * @param  Thaut_ticks : durée de l'état haut d'une imp
                       ulsion en Ticks
   14 00000000         ;  * @retval None
   15 00000000         ; */
   16 00000000         
   17 00000000         ;void PWM_Set_Value_TIM3_Ch3( unsigned short int Thaut_t
                       icks);
   18 00000000                 import           PWM_Set_Value_TIM3_Ch3
   19 00000000         
   20 00000000         
   21 00000000         
   22 00000000         ;/**
   23 00000000         ; * @brief  Mise à 1 d'une broche GPIO 
   24 00000000         ;  * @note   Une fonction par GPIO
   25 00000000         ; * @param  Broche : 0 à 15
   26 00000000         ; * @retval None
   27 00000000         ; */
   28 00000000         
   29 00000000         ;void GPIOA_Set(char Broche);
   30 00000000                 import           GPIOA_Set
   31 00000000         
   32 00000000         ;void GPIOB_Set(char Broche);
   33 00000000                 import           GPIOB_Set
   34 00000000         
   35 00000000         ;void GPIOC_Set(char Broche);
   36 00000000                 import           GPIOC_Set
   37 00000000         
   38 00000000         
   39 00000000         
   40 00000000         ;/**
   41 00000000         ; * @brief  Mise à 0 d'une broche GPIO 
   42 00000000         ;  * @note   Une fonction par GPIO
   43 00000000         ; * @param  Broche : 0 à 15
   44 00000000         ; * @retval None
   45 00000000         ;  */
   46 00000000         
   47 00000000         ;void GPIOA_Clear(char Broche);
   48 00000000                 import           GPIOA_Clear
   49 00000000         



ARM Macro Assembler    Page 2 


   50 00000000         ;void GPIOB_Clear(char Broche);
   51 00000000                 import           GPIOB_Clear
   52 00000000         
   53 00000000         ;void GPIOC_Clear(char Broche);
   54 00000000                 import           GPIOC_Clear
   55 00000000         
   56 00000000                 end
    4 00000000         
    5 00000000         ; ====================== zone de réservation de données,
                         ======================================
    6 00000000         ;Section RAM (read only) :
    7 00000000                 area             mesdata,data,readonly
    8 00000000         
    9 00000000         
   10 00000000         ;Section RAM (read write):
   11 00000000                 area             maram,data,readwrite
   12 00000000 00000000 
                       FlagCligno
                               dcd              0
   13 00000004         
   14 00000004         
   15 00000004         ; ======================================================
                       =========================================
   16 00000004         
   17 00000004         
   18 00000004         
   19 00000004         
   20 00000004         ;Section ROM code (read only) :  
   21 00000004                 area             moncode,code,readonly
   22 00000000         
   23 00000000         
   24 00000000                 export           FlagCligno
   25 00000000                 export           timer_callback
   26 00000000         
   27 00000000         ; écrire le code ici
   28 00000000         timer_callback
                               proc
   29 00000000         
   30 00000000 B500            push             {lr}
   31 00000002         ;r1 : &FlagCligno
   32 00000002 4909            ldr              r1, =FlagCligno
   33 00000004         ; r2 : * (&FlagCligno)
   34 00000004 680A            ldr              r2, [r1]
   35 00000006 3A01            subs             r2, #1
   36 00000008         
   37 00000008 D107            bne              Action1
   38 0000000A         ; on met la valeur 0 dans r0
   39 0000000A F04F 0000       mov              r0, #0
   40 0000000E         ; on stocke à l'adresse r1 la valeur dans r0
   41 0000000E 6008            str              r0, [r1]
   42 00000010         ;on prépare R0 pour l'appel de la fonction
   43 00000010 F04F 0001       mov              r0, #1
   44 00000014 F7FF FFFE       bl               GPIOB_Set
   45 00000018 D104            bne              Fin
   46 0000001A         
   47 0000001A         Action1
   48 0000001A         ; on met la valeur 1 dans r0
   49 0000001A F04F 0001       mov              r0, #1
   50 0000001E         ; on stocke à l'adresse r1 la valeur dans r0



ARM Macro Assembler    Page 3 


   51 0000001E 6008            str              r0, [r1]
   52 00000020         ;on a r0 à 1 pour l'appel de la fonction
   53 00000020 F7FF FFFE       bl               GPIOB_Clear
   54 00000024         
   55 00000024         Fin
   56 00000024 BD00            pop              {pc}
   57 00000026                 endp
   58 00000026         
   59 00000026         
   60 00000026         
   61 00000026         
   62 00000026         
   63 00000026         ;/*
   64 00000026         ;void timer_callback(void)
   65 00000026         ;{
   66 00000026         ; if (FlagCligno==1)
   67 00000026         ; {
   68 00000026         ;  FlagCligno=0;
   69 00000026         ;  GPIOB_Set(1);
   70 00000026         ; }
   71 00000026         ; else
   72 00000026         ; {
   73 00000026         ;  FlagCligno=1;
   74 00000026         ;  GPIOB_Clear(1);
   75 00000026         ; }
   76 00000026         ;}*/
   77 00000026         
   78 00000026                 END
              00 00 00000000 
Command Line: --debug --xref --diag_suppress=9931 --cpu=Cortex-M3 --apcs=interw
ork --depend=.\obj\cligno.d -o.\obj\cligno.o -I.\Driver -I.\RTE\_Simu -IC:\Prog
ramdata\Keil\Arm\Packs\ARM\CMSIS\5.7.0\CMSIS\Core\Include -IC:\Programdata\Keil
\Arm\Packs\Keil\STM32F1xx_DFP\2.3.0\Device\Include --predefine="__EVAL SETA 1" 
--predefine="__MICROLIB SETA 1" --predefine="__UVISION_VERSION SETA 534" --pred
efine="_RTE_ SETA 1" --predefine="STM32F10X_MD SETA 1" --predefine="_RTE_ SETA 
1" --list=cligno.lst Src\Cligno.s



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

mesdata 00000000

Symbol: mesdata
   Definitions
      At line 7 in file Src\Cligno.s
   Uses
      None
Comment: mesdata unused
1 symbol



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

FlagCligno 00000000

Symbol: FlagCligno
   Definitions
      At line 12 in file Src\Cligno.s
   Uses
      At line 24 in file Src\Cligno.s
      At line 32 in file Src\Cligno.s

maram 00000000

Symbol: maram
   Definitions
      At line 11 in file Src\Cligno.s
   Uses
      None
Comment: maram unused
2 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

Action1 0000001A

Symbol: Action1
   Definitions
      At line 47 in file Src\Cligno.s
   Uses
      At line 37 in file Src\Cligno.s
Comment: Action1 used once
Fin 00000024

Symbol: Fin
   Definitions
      At line 55 in file Src\Cligno.s
   Uses
      At line 45 in file Src\Cligno.s
Comment: Fin used once
moncode 00000000

Symbol: moncode
   Definitions
      At line 21 in file Src\Cligno.s
   Uses
      None
Comment: moncode unused
timer_callback 00000000

Symbol: timer_callback
   Definitions
      At line 28 in file Src\Cligno.s
   Uses
      At line 25 in file Src\Cligno.s
Comment: timer_callback used once
4 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
External symbols

GPIOA_Clear 00000000

Symbol: GPIOA_Clear
   Definitions
      At line 48 in file .\Driver\DriverJeuLaser.inc
   Uses
      None
Comment: GPIOA_Clear unused
GPIOA_Set 00000000

Symbol: GPIOA_Set
   Definitions
      At line 30 in file .\Driver\DriverJeuLaser.inc
   Uses
      None
Comment: GPIOA_Set unused
GPIOB_Clear 00000000

Symbol: GPIOB_Clear
   Definitions
      At line 51 in file .\Driver\DriverJeuLaser.inc
   Uses
      At line 53 in file Src\Cligno.s
Comment: GPIOB_Clear used once
GPIOB_Set 00000000

Symbol: GPIOB_Set
   Definitions
      At line 33 in file .\Driver\DriverJeuLaser.inc
   Uses
      At line 44 in file Src\Cligno.s
Comment: GPIOB_Set used once
GPIOC_Clear 00000000

Symbol: GPIOC_Clear
   Definitions
      At line 54 in file .\Driver\DriverJeuLaser.inc
   Uses
      None
Comment: GPIOC_Clear unused
GPIOC_Set 00000000

Symbol: GPIOC_Set
   Definitions
      At line 36 in file .\Driver\DriverJeuLaser.inc
   Uses
      None
Comment: GPIOC_Set unused
PWM_Set_Value_TIM3_Ch3 00000000

Symbol: PWM_Set_Value_TIM3_Ch3
   Definitions
      At line 18 in file .\Driver\DriverJeuLaser.inc
   Uses
      None
Comment: PWM_Set_Value_TIM3_Ch3 unused
7 symbols
351 symbols in table
